---
type: note
tags: [note]
created: 2025-11-10T22:06:49.803Z
updated: 2025-11-15T20:19:57.210Z
---# Sennheiser G3 wireless transmitter-receiver

Sennheiser system operating at 544.450 MHz falls within the legal UHF range in Canada — specifically within the H10 band (542–572 MHz), which is approved for license-exempt wireless microphone use.

wireless bodypack by Sennheiser that is in a frequency range B 626-668 MHz. SK 100

Diversity Receiver EK 100 frequency range B 626-668 MHz

## Links

- [boxi.DEVICES: SennheiserEW100G3WirelessUserGuide.pdf](localexplorer:Z:\SENNHEISER G3 Wireless Kit\SennheiserEW100G3WirelessUserGuide.pdf)
- [ISED: ](https://ised-isde.canada.ca/site/spectrum-management-telecommunications/en/learn-more/key-documents/spectrum-advisory-bulletins-sab/sab-003-17-low-power-radio-apparatus-including-wireless-microphones-band-614-698-mhz)
- [sennheiser.com](https://www.sennheiser.com)


---
**Keywords:** note
