Video Color Setup
December 24, 2021
5:33 PM
C-log
8 bit 
LUT BT2020_CanonLog-to-BT709
Shoot c-log or c-log 3 on EOS R?

Clog minimum iso 400, clog3 800. Maybe in low light or low dynamic range situations, clog has an edge in noise? Also it is supposed to be easier to grade.
I did a test yesterday night indoors, with clog and clog3, with all the different color gamuts (bt709, bt2020 and cinema gamut only in clog3), and after applying the corresponding Canon original lut, all the clips looked pretty much the same.
The only difference is Clog with the EOS Original matrix. When I tested my old Eos R outdoors in daylight I found I liked better this Eos original matrix over the neutral one. Interestingly, you can't choose this matrix with clog3...
From <[link]> 