Avid DNxHR - Digital Nonlinear Extensible High Resolution
April 13, 2022
5:08 PM
DNxHR
Preliminary Specifications[edit]
DNxHR is available in the following flavors:[2][3]
DNxHR LB - Low Bandwidth (8-bit 4:2:2) Offline Quality
DNxHR SQ - Standard Quality (8-bit 4:2:2) (suitable for delivery format)
DNxHR HQ - High Quality (8-bit 4:2:2)
DNxHR HQX - High Quality (12-bit 4:2:2) (UHD/4K Broadcast-quality delivery)
DNxHR 444 - Finishing Quality (12-bit 4:4:4) (Cinema-quality delivery)
Bandwidth requirements for the codec and its different flavors have been announced in the "Avid High Resolution Workflows Guide - December 2014" on page 111.[2]
Updated August 2015 avid.force.com "DNxHR Codec Bandwidth Specifications".[3]
From <[link]> 