CRF scale between
March 20, 2022
5:54 PM
The range of the CRF scale is 0–51, where 0 is lossless (for 8 bit only, for 10 bit use -qp 0), 23 is the default, and 51 is worst quality possible. A lower value generally leads to higher quality, and a subjectively sane range is 17–28. Consider 17 or 18 to be visually lossless or nearly so; it should look the same or nearly the same as the input but it isn't technically lossless